August 04, 2025

Pope

ATTN: Contact Person

Quote #: Pope ZF080425E

# Subject: LT9000 Level Transmitter

We are pleased to quote on the following equipment for your upcoming applications:

1 QTY LT9000-115VAC-H-10" LEVEL TRANSMITTER $1060.00 EACH

* Continuous Level Transmitter
* Supply Voltage: 115VAC
* Output: 4 to 20mA
* Process Connection: 3/4" NPT, 316SS ( Max.)
* Insulator: Teflon, 4 (450 F)
* Probe: ½" Diameter Halar Coated x 10"
* Housing: Cast Aluminum, NEMA 7, D; NEMA 9, E, F, & G
* 2-Year Warranty

Delivery: In Stock FCA; Factory, Houston, TX

Terms: Net 30 days W.A.C. or CC Quotation valid for 30 days.

**APPLICATION NOTES**

**THE LT 9000 IS DESIGNED TO BE USED IN ELECTRICALLY CONDUCTIVE LIQUIDS THAT DO NOT LEAVE A RESIDUE ON THE PROBE.** A wet electrically conductive coating will give an indication of level at the highest point that there is a continuous coating from the surface of the fluid.

The LT 9000 will give a varying output, if the conductivity of the material changes.

For proper operation, the LT 9000 must be grounded to the fluid. In non-metallic tanks, extra grounding provisions may be necessary. It is good engineering practice to provide a separate independent high-level alarm in critical applications, rather than using a set point based on the 4-20mA output.

Please contact me directly if you have any questions or require more information.

Thank you,

Zoe Fleming

(713) 467-4438

Zoe@babbittt.us