{{date}}

{{customer\_name}}

**ATTN:** {{attention\_name}}

**Quote #:** {{quote\_number}}

Subject: LS2100 Level Switch – Loop Power

{{quantity}} QTY {{**part\_number**}}{{unit\_price}} EACH

* Supply Voltage: 16 TO 32 VDC
* Output: Normal 8mA; Alarm 16mA
* Field reversible output
* Process Connection: {{pc\_size}} {{pc\_rate}} {{pc\_type}}, {{pc\_matt}} ({{max\_pressure}} Max.)
* Insulator: {{ins\_material}}, {{ins\_length}} ({{ins\_temp}} F)
* Probe: {{probe\_size}}" Diameter {{probe\_material}} x {{probe\_length}}"
* Housing: Cast Aluminum, NEMA 7, C, D; NEMA 9, E, F, & G
* 2 Year Warranty

Notes:

* Other supply voltages available at no extra charge
* Special materials of construction – please call factory

Delivery: {{lead\_time}} FOB; Houston, TX

Terms: NET W.A.C. Quotation valid for 30 days.

Please contact me directly if you have any questions or require more information.

Thank you,

{{employee\_name}}

{{employee\_phone}}

{{employee\_email}}

[www.babbittinternational.com](http://www.babbittinternational.com/)