{{date}}

{{customer\_name}}

**Attn:** {{attention\_name}} **Quote #:** {{quote\_number}}

Subject: Quotation for FS10000 Dry Material Flow Switch

{{quantity}} QTY **{{part\_number}} w/ 15 feet of cable** $ {{unit\_price}} EACH

* Supply Voltage: {{supply\_voltage}} Electronics mounted in

a non-metallic 10” x 8” x 5” NEMA 4X

enclosure w/ clear acrylic window.

* Output: 5 Amp DPDT Relay
* Adjustable time delay
* Process Connection: {{pc\_size}} {{pc\_rate}} {{pc\_type}}, {{pc\_matt}}
* Insulator: {{ins\_material}}, {{ins\_length}} {{ins\_long}} ({{ins\_temp}} F)
* Probe: {{probe\_size}}" Diameter {{probe\_material}} x {{probe\_length}}"
* Housing: Cast Aluminum, NEMA 7, C, D; NEMA 9, E, F, & G
* 15 feet Coaxial Cable w/ Connectors
* 2 Year Warranty

NOTES:

* Max probe length is 24”
* For detecting emissions before they are visible, we recommend air velocities of 2000 feet per minute or greater.

Delivery: 3 to 5 Days FOB; Houston, TX

Terms: NET 30 W.A.C. Quotation valid for 30 days.

Thank you,

{{employee\_name}}

{{employee\_phone}}

{{employee\_email}}

[www.babbittinternational.com](http://www.babbittinternational.com/)