July 09, 2025

ACME

ATTN: Jimmy Quote #: Q-20250709-0740

Subject: LS2000 Level Switch Quote

1 QTY LS2000-115VAC-H-10" $Please Contact EACH

* Supply Voltage: 115VAC
* Output: 10 Amp SPDT Relay
* Selectable Fail-Safe High or Low Level
* Process Connection: ¾” NPT, 316SS (300 PSI Max.)
* Insulator: UHMPE, 4” Long (180 F)
* Probe: ½” Diameter 316SS x XX” (Including Insulator)
* Housing: Cast Aluminum, NEMA 7, C, D; NEMA 9, E, F, & G
* 2-Year Warranty

Notes:

* For longer probes please add $ 45.00 per foot
* Other supply voltages available at no extra charge
* Special materials of construction – please call factory

Delivery: FOB; Houston, TX

Terms: NET 30 W.A.C. Quotation valid for 30 days.

Please contact me directly if you have any questions or require more information.

Thank you,

John Nicholosi

(713) 467-4438

John@babbitt.us

[www.babbittinternational.com](http://www.babbittinternational.com/)