Babbitt International

# Point Level Switch Quote

**Part Number:** LS2000-115VAC-S-10"-XSP-VR-8"TEFINS **Date:** August 04, 2025

============================================================

## Product Information

|  |  |
| --- | --- |
| Specification | Value |
| Model | LS2000 |
| Voltage | 115VAC |
| Probe Material | 316 Stainless Steel |
| Probe Length | 10.0" |
| Housing | Cast Aluminum, NEMA 7, C, D; NEMA 9, E, F, & G |
| Output | 10 Amp SPDT Relay |

## Technical Specifications

### Process Connection

**Type:** NPT  
**Size:** 3/4"  
**Material:** S

### Insulator

**Material:** Teflon  
**Length:** 8.0"

### Operating Limits

**Max Temperature:** 450°F  
**Max Pressure:** 300 PSI  
**O-Ring Material:** Viton

## Options

* **XSP:** Extra Static Protection
* **VR:** Vibration Resistance

============================================================

*Generated by Babbitt Quote Generator v1.0  
Generated on: August 04, 2025 at 01:00 AM*

**Babbitt International**www.babbittinternational.com