August 04, 2025

Customer Name

Attn: Contact Person

Quote #: CUSTOMER ZF080425C

Subject: Quotation for FS10000 Dry Material Flow Switch

1 QTY FS10000-115VAC-S-6" w/ 15 feet of cable $1920.00 EACH

* Supply Voltage: 115VAC Electronics mounted in a non-metallic 10” x 8” x 5” NEMA 4X enclosure w/ clear acrylic window.
* Output: 5 Amp DPDT Relay
* Adjustable time delay
* Process Connection: 3/4" NPT, 316SS
* Insulator: UHMWPE, 2 (180 F)
* Probe: ½" Diameter 316 Stainless Steel x 6.0"
* Housing: Cast Aluminum, NEMA 7, C, D; NEMA 9, E, F, & G
* 15 feet Coaxial Cable w/ Connectors
* 2 Year Warranty

Notes:

* Max probe length is 24”
* For detecting emissions before they are visible, we recommend air velocities of 2000 feet per minute or greater.

Delivery: In Stock FOB; Houston, TX

Terms: NET 30 W.A.C. Quotation valid for 30 days.

Thank you,

Zoe Fleming

(713) 467-4438

Zoe@babbittt.us

[www.babbittinternational.com](http://www.babbittinternational.com/)