August 04, 2025

Pope

ATTN: Contact Person Quote #: Pope ZF080425B

Subject: LS2100 Level Switch – Loop Power

1 QTY LS2100-24VDC-S-10" $ $520.00 EACH

* Supply Voltage: 16 TO 32 VDC
* Output: Normal 8mA; Alarm 16mA
* Field reversible output
* Process Connection: 3/4" NPT, 316SS (300 PSI Max.)
* Insulator: Teflon, 4.0 4.0" Teflon (450 F)
* Probe: ½" Diameter 316 Stainless Steel x 10.0"
* Housing: Cast Aluminum, NEMA 7, C, D; NEMA 9, E, F, & G
* 2 Year Warranty

Notes:

* Other supply voltages available at no extra charge
* Special materials of construction – please call factory

Delivery: In Stock FOB; Houston, TX

Terms: NET W.A.C. Quotation valid for 30 days.

Please contact me directly if you have any questions or require more information.

Thank you,

Zoe Fleming

(713) 467-4438

Zoe@babbittt.us

[www.babbittinternational.com](http://www.babbittinternational.com/)