August 04, 2025

Pope

ATTN: Contact Person

Quote #: Pope ZF080425F

Subject: LS7000 Level Switch Quote

1 QTY LS7000-115VAC-S-10" $715.00 EACH

* Supply Voltage: 115VAC
* Output: 2 Form C contacts 5 Amp DPDT Relay
* Selectable Fail-Safe High or Low Level
* Adjustable Time Delay
* Built-in Fuse
* Process Connection: 1" NPT, 316SS (1500 PSI Max.)
* Insulator: Teflon, 4 (450 F)
* Probe: ½" Diameter 316 Stainless Steel x 10"
* Housing: Cast Aluminum, NEMA 7, D; NEMA 9, E, F, & G
* 2-Year Warranty

Notes:

* Other supply voltages available at no extra charge
* Special materials of construction – please call factory

Delivery: In Stock FOB; Houston, TX

Terms: NET 30 W.A.C. Quotation valid for 30 days.

Please contact me directly if you have any questions or require more information.

Thank you,

Zoe Fleming

(713) 467-4438

Zoe@babbittt.us

[www.babbittinternational.com](http://www.babbittinternational.com/)