July 14, 2025

New Customer

ATTN: Contact Person Quote #: ZF071425B

Subject: LS2100 Level Switch – Loop Power

1 QTY LS2100-24VDC-S-10" $ 520.00 EACH

* Supply Voltage: 16 TO 32 VDC
* Output: Normal 8mA; Alarm 16mA
* Field reversible output
* Process Connection: 3/4" NPT, 316SS (300 PSI Max.)
* Insulator: Teflon, 4" Long (450 F)
* Probe: ½" Diameter 316 Stainless Steel x 10"
* Housing: Cast Aluminum, NEMA 7, C, D; NEMA 9, E, F, & G
* 2 Year Warranty

Notes:

* For longer probes please add $ 45.0 per foot
* Other supply voltages available at no extra charge
* Special materials of construction – please call factory

Delivery: FOB; Houston, TX

Terms: NET W.A.C. Quotation valid for 30 days.

Please contact me directly if you have any questions or require more information.

Thank you,

Zoe Fleming

(713) 467-4438

zoe@babbitt.us

[www.babbittinternational.com](http://www.babbittinternational.com/)