{{date}}

{{customer\_name}}

**ATTN:** {{attention\_name}}

**Quote #:** {{quote\_number}}

Subject: LS8000/2 Level Switch

{{quantity}} QTY {{**part\_number**}}{{unit\_price}} EACH

* Snap Track Mounted Remote Electronics
* Supply Voltage: {{supply\_voltage}}
* Output: 3 10 Amp SPDT Relay
* Selectable Fail-Safe High or Low Level
* Built-in Fuse
* Process Connection: {{pc\_size}} {{pc\_rate}} {{pc\_type}}, {{pc\_matt}} ({{max\_pressure}} Max.)
* Insulator: {{ins\_material}}, {{ins\_length}} ({{ins\_temp}} F)
* Probe: {{probe\_size}}" Diameter {{probe\_material}} x {{probe\_length}}"
* Probe Housing: Cast Aluminum, NEMA 7, C, D; NEMA 9, E, F, & G
* 2-Year Warranty

Notes:

* Other supply voltages available at no extra charge
* Special materials of construction – please call factory

Delivery: {{lead\_time}} FOB; Houston, TX

Terms: NET 30 W.A.C. Quotation valid for 30 days.

Please contact me directly if you have any questions or require more information.

Thank you,

{{employee\_name}}

{{employee\_phone}}

{{employee\_email}}

[www.babbittinternational.com](http://www.babbittinternational.com/)