DATE: {{quote\_date}}

{{cust\_company}}

**ATTN:** {{cust\_name}} **Quote #:** {{quote\_num}}

Subject: {{family}}

{{p1\_qty}} QTY {{p1\_name}}{{p1\_price}} EACH

* Supply Voltage: {{voltage}}
* Output: 10 Amp SPDT Relay
* Selectable Fail-Safe High or Low Level
* Process Connection: {{product\_1\_connection}}, {{produc\_1\_connection\_material}} (300 PSI Max.)
* Insulator: Teflon, 4” Long (450 F)
* Probe: ½” Diameter HALAR x XX” (Including Insulator)
* Housing: Cast Aluminum, NEMA 7, C, D; NEMA 9, E, F, & G
* 2-Year Warranty

Notes:

* For longer probes please add $ 110.00 per foot
* Other supply voltages available at no extra charge
* Special materials of construction – please call factory

Delivery: FOB; Houston, TX

Terms: NET 30 W.A.C. Quotation valid for 30 days.

Please contact me directly if you have any questions or require more information.

Thank you,

{{sales\_name}}

{{sales\_phone}}

{{sales\_email}}

[www.babbittinternational.com](http://www.babbittinternational.com/)