August 04, 2025

ACME Industrial Solutions

ATTN: John Smith, P.E. Quote #: Q-2024-UNIFIED-SINGLE-001

Subject: LS2000 Level Switch Quote

2 QTY LS2000-115VAC-S-12 $ 1,250.00 EACH  
  
• Supply Voltage: 115VAC  
• Output: 10 Amp SPDT Relay  
• Fail-Safe: Selectable Fail-Safe High or Low Level  
• Process Connection: ¾" 300 PSI NPT, SS (300 PSI Max.)  
• Insulator: UHMWPE, 4" Long (450 F)  
• Probe: ½" Diameter 316SS x 12"  
• Housing: Cast Aluminum, NEMA 7, C, D; NEMA 9, E, F, & G  
• Warranty: 2-Year Warranty

Delivery: 6-8 weeks FOB; Houston, TX

Terms: NET 30 W.A.C. Quotation valid for 30 days.

Please contact me directly if you have any questions or require more information.

Thank you,

John Nicholosi

(713) 467-4438

John@babbitt.us

[www.babbittinternational.com](http://www.babbittinternational.com/)